# Dashboard Tab

If for selected parameter, sampling Technique is ‘Sampling’ then Tab caption will display ‘Cp/Cpk’

If for Sampling Technique is ‘100% Inspection’ tab caption will display ‘Pp/Ppk’

For mixed parameter tab caption will display ‘Cp/Cpk’.

Displaying Cp, Cpk or Pp, Ppk value on button check-

- The value is below of configure Cpk or Ppk value (in trend setting screen) if it is less then that button will display in Red color and in feedback Red light will get display.

- The value is above of configure Cpk or Ppk value (in trend setting screen) if it is greater then that button will display in Green color and in feedback Green light will get display.

Total Parameters to be display –

- If parameter count is greater than entered value in ‘Total parameter to be display’ textbox then Next button will get enabled.

- If parameter count is less than entered or available value in textbox then Prev & next button will get disabled.

- Maximum 12 parameters will get display.

# Cp, Cpk or Pp, Ppk Value {Based on Last SampleNo] –

On dashboard Tab, for a parameter ‘Display Cpk or Ppk value’ to zero then system will calculate the Cp, Cpk or Pp, Ppk for all sample no and for greater than zero then system will calculate Cp, Cpk or Pp, Ppk based on last sample no. Process Status will also display the color depends upon the Display Cpk or Ppk value in Dashboard for last sample numbers.

# Cp/Cpk Display on Display Board –

After completion of each sample or after every reading for each parameter Cp, Cpk, Pp, Ppk (whichever is configure in Configurable Parameter) is to be display on display board