# Fixture Mapping

This screen provides you a facility to record the readings for various parameters of a part in a single go using fixtures. All the fields on this screen are mandatory. You may enter the information in the following fields by selecting appropriate values from the drop-down list

Fixture code

Part code

Process code

Parameter code

Sequence no.

Formulae

Master Value

Reading type

Fixture Mapping allows mapping parts defined in Standard QAP. Formulae for parameter can be defined by using probes available in selected fixture. Initially setting value set for Part-Process-Parameter in Standard QAP will be shown in Master Value text box. Master value can be changed before saving. Reading Type can be STATIC, MIN, MAX, AVG, TIR this field decides type of reading that needs to be recorded against parameter.

You can modify only the Formulae, Master Value, Sequence Number and Reading Type for selected Fixture, Part, Process and Parameter. Grid will display details such as Parameter Code, Description, and Sequence No, Formulae, Master Value and Reading Type for only those parameters, which have been already mapped to selected Fixture, Part and Process

For deleting a record, you have to select Fixture Code, Part Code, Process Code and Parameter Code from the drop down lists. If the record is referenced then message will be displayed to the user stating that the record is being referenced in Job.