# Fixture Measuring (Gauge Repeatability & Reproducibility) screen

This screen is used to capture the readings for the parameters. Readings can be taken for any part no randomly. You have to select the part no from the Part No drop down list box before capturing the readings. Click on the Start button or the hardware switch (i.e. foot switch or hand switch), readings for the parameters shall be displayed in the text boxes. Click on the Stop button to store the reading for the Part No. You may select part no’s from the drop down list box and continue the above-mentioned procedure to capture the readings. On completion of readings for the 10 part no’s, click the Save & Close button to save the readings. This one set of readings for 10 part no.’s is known as a trial. If the caption of the Start/Stop button is Start then you may click the Cancel button to discard the readings and close the screen. If the caption of the Start/Stop button is Stop then you may click the Cancel button to reset the readings from the probes in case of Dynamic parameters.