# Measurement

The Data Capturing and Data Analysis screen is launched when you click Measure on the Reading tab of the Local Monitoring screen.

Use this screen for:

Recording data for multiple Variable parameters for multiple jobs manually or automatically.

- Viewing Trends which occur during capture of data.

- Viewing Charts for Data Analysis.

- Viewing Control Charts along with the Statistical Analysis for single Parameter

- View Bar Display

- Viewing Cp/Cpk or Pp/Ppk value (Dash Board)

This screen has six tabs –

Readings tab

Charts tab

Control Chart tab

Bar Display Tab

Dashboard tab

Component Tab

Bar display, Dash Board tab and Component tab will get display depending upon the Configuration setting.

After measurement screen get launch and job is of Esya Instrument, request will send to Instrument by using the Instrument address of the parameter, for collecting the data after each 20 sec. During dumping a data, system will check send & received command address is same or Not if it is different the log file will get updated for send & received command address.

Data will get stored only when the reading number is different than earlier. Example – Instrument return COYR1+000.487, system will check Reading No 1 is last reading No for selected parameter, If yes then system will not dump the data/reading If no data will get stored in the respective parameter.

Close button will get disable during sending a request. After finishing the request for all parameter Close button will get enabled.