# Dashboard_CpCpk_Screen

It displays Job related parameters information for selected cell/location gets display.

This Page has Job No, Machine No., Part No, Parameter, Process Status, Cp and Cpk.

- When Parameter is 100% inspection then display the value of Pp, Ppk.

- When Parameter is sampling then display the value of Cp, Cpk.

- When Parameters are only 100% inspection then display the header is Pp, Ppk.

- When Parameters are Sampling and 100% Inspection then display the header is Cp, Cpk.

Process status will display the color depending upon the Control Limits and Cpk or Ppk value from XBarRSetting. If Cpk or Ppk value is blank from XBarRSetting then Cpk or Ppk value will be considered as 1.66

- In Control means - Xbar of sample is within control Limit

- Not in Control - Xbar of sample is Out of control Limit

- Capable - Cpk > 1.66

- Not Capable - Cpk < 1.66

Process Status will have color Green when Process Status is In Control & Capable.

Process Status will have color Yellow when Process Status is Not In Control but Capable.

Process Status will have color Orange when Process Status is In Control & Not Capable.

Process Status will have color Red when Process Status is Not in Control & Not Capable.

Some samples has been taken and when user click on Process Status for that parameter then user can see the Control Charts in different page for the selected parameter. Sample has not been taken and when user click on Process Status for that parameter then display the message ‘No Reading taken’. When reading has not taken for a particular parameter then the Process status will be disabling and display the default color i.e. other than Green, Yellow, Orange and Red.

If user configure ‘Display Cpk or Ppk value’ to zero (0) in Job Creation then Cp, Cpk or Pp, Ppk value will be calculated and display for all samples.

If user put the sample no 20 then system will calculate for last 20 samples.