# Reading Modes of Measure Screen

Reading Mode for capturing data can be Manual or Automatic.

In case of Manual Mode – Data entered in reading text box is saved into database. Reading entered in text box is dumped into database on pressing the Enter Key.

In case of Automatic Mode – Data is captured based on instrument and interface selected. Various interfaces, which are allowed through PROQMS, are

PMDI – 8 Channel Interface

PMDI – 16 Channel Interface

WB – Weighing Balance

BK941 – Baker 941 unit

BKCALP – Baker Caliper

In case of Automatic Mode, if the instruments selected are due for calibration then the message "Instrument(s) due for calibration Instrument Number" is displayed.