# Specification Limits

The engineering requirement for judging acceptability of a particular characteristic. A specification is never to be confused with a control limit. Ideally specification ties directly to or is compatible with the customer’s requirements or expectations. User can modify LSL, USL, Nominal value, Sample size and Frequency of more than one parameter through this screen.

When the user click on Specs Limit button then Change Specification Limit screen will get display. Instrument address column get visible only in the grid for process-parameter having interface code as ‘ESYA’. User can see all parameters instrument address through this screen.

Cpk for Sample No’s should not be blank but can be zero.