# Sampling

You may set size of the sample for quality measurement in the Sample Size text box. You may also specify how frequently sample size may be collected in the Sample Frequency text box.

The manufactured parts may undergo either 100% Inspection or you may choose to do Sampling for the measurement of quality. This may be chosen from the Sampling Technique group box. You may select either Sampling or 100% inspection. If Attributive option is selected in the Parameter tab then you have to enter the Subgroup Size. If subgroup size is not fixed, 0 can be entered in Subgroup Size text box

In mode ‘A’ and ‘M’ when the sampling technique is 100% inspection, sample frequency (in min) should be enabled