# Data Capturing

Reading – ((Calculated as per formulae of parameter + Calibration Value) * Gain Factor) + Master Value

In case of Dynamic parameter caption of switch will be "Stop" and no readings are captured from connected probes. For capturing readings press on Stop button or press H/W switch caption of button will be changed to Start and system will start capturing readings from connected probes and it will first evaluate formulae by considering probe readings then will calculate reading as per Reading explained above. After calculating reading, the system will compare this reading with the previous calculated readings and then the latest readings will be shown in current reading text box .On click of Start button system will dump reading of parameter(s) into database and caption will be set back to Stop and no readings are captured.

In case of Static parameters caption of button will be always Start and system is continuously capturing probe values and by using this it will evaluate formulae of parameter and then it will calculate reading as per Reading as explained above. Reading calculated is final reading and it will be shown in current reading text box. On click of Start button or press of H/W switch system will dump readings into database the caption of button will be Start.