# The Bar Display tab (Measurement)

Bar Display tab will display one bar for each parameter selected from Local Monitor screen. It will display Bar image, Reading, USL, LSL, Parameter and the process vertically (one below the other).

If reading is less than LSL, bar will be displayed with Yellow Color.

If reading is Greater than USL, Bar will be displayed with Red Color.
If reading is within Specification Limit, Bar will display Green Color

Top portion of the Bar Display Tab will display following information: -

Operation – Display Location from Machine Master for machine set for selected job/s. [Location]

Machine – Display Machine from Job.

Die Code - Die Code that has been set for Part-Machine of selected Jobs otherwise NA

Comp. Code – Part Code field from Part Master screen.

Revision No & Date - Drawing File field from Part Master screen.

Insp. Name – Login Name

Supr. Name – Supervisor Name combo box will be enabled and non editable

User can view Only 28 parameters because of the limitation of the Screen width